{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":9,"rows_kept":8,"merged":[[0,0,0,8],[3,0,3,6],[4,0,4,6],[5,0,5,6],[6,0,6,4],[6,5,6,8],[7,0,7,8]]}
["四川省区域应急救援雅安基地项目柴油发电机采购安装清单"]
["序号","名称","规格型号","单位","数量","不含税控制单价（元）","不含税单价（元）","不含税金额（元）","备注"]
[1,"柴油发电机组","柴油发电机组\n2.型号、规格、技术参数：柴油发电机组 常用功率1500KW\n3.含自启动柴油发电机组、发电机自带控制柜设备、蓄电池,油机启动柜自带出线保护开关,带减震系统 、油箱油泵、空气滤清器、机房烟尘处理器、尾气净化系统、散热器、排烟管、排烟阀、消声器、油箱通气管、等符合规范要求\n4.包括基础、型钢、减震处理、预埋件、接地,油箱及柴油,输油管道,蓄电池箱及相关构件安装\n5.除尘、降噪及隔音、废气处理等均通过环保验收及相关政府部门验收\n6.满足招标、施工验收规范及建设方品牌、技术标准要求等，包括发电机本身、检查接线、本体调试、发电机尾气净化系统及技术要求配套的全部内容\n7.与低压开关柜间的自启动管线综合考虑\n8.其他：满足设计、相关图集、标准及招标技术要求","台",1,845575.22,null,null,"不需要施工吸音墙体；厂方必须现场测试发电机功率，带够1500kw的负载，并承担所有的费用。"]
["暂估不含税合计（元）"]
["税率：",{"$nulls":6},"%"]
["暂估含税合计（元）"]
["报价单位名称（加盖公章）：",{"$nulls":4},"联系人及联系电话："]
["注：报价采用固定综合单价。供应商根据清单及图纸自主综合考虑报价，报价保留小数点后两位。报价包含但不限于主材费用、辅材费用、耗材费用、损耗费用、运送费、二次搬运费、二次深化设计费用、卸车、人工费用、资料费、管理费、竣工验收费、材料及分包工程验收试验检测费用、安全文明施工费、措施项目费、赶工费用、成品保护费、供应商人员薪资和意外伤害保险费、工人食宿费用、供应商合理利润、完工后清洁工作相关费用、不可预见费用等供应商一切直接和间接费用。至工程完工期间出现的人工、材料等费用的上涨，属于供应商承担的风险范畴，价款均不予调整。具体金额以实际结算金额为准。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}