{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"merged":[[0,0,0,10],[21,0,21,4],[21,5,21,10],[22,0,22,10]]}
["雅安市雨城区人民医院能力建设二期项目灯具、开关材料采购清单"]
["序号","货物名称","主要技术指标（参数）","单位","数量","含税单价（元）","不含税单价（元）","不含税合价（元）","税率","含税合价（元）","备  注"]
[1,"LED平板灯","38W;600*600;4200K、芯片：OSRAM Ra≧90.R9=51 开孔585*585、IP等级：IP20、发光角度：120度","个",800]
[2,"LED平板灯（带蓄电池）","38W;600*600;4200K、芯片：OSRAM Ra≧90 R9=51 IP等级：IP20、发光角度：120度","个",100]
[3,"LED筒灯","9w φ100 4200k、芯片：OSRAM Ra≧90 R9=51 IP等级：IP20、","个",450]
[4,"圆形平板灯","36w 600*600 4200k、芯片：OSRAM Ra≧90 R9=51 开孔585*585、IP等级：IP20、发光角度：120度","个",120]
[5,"吸顶灯（铝扣板）","12w 300*300 4200k、芯片：OSRAM Ra≧90  R9=51 IP等级：IP20、发光角度：120度","个",200]
[6,"圆形吸顶灯（带蓄电池）","12w 300*300 4200k、芯片：OSRAM Ra≧90 R9=51 IP等级：IP20、发光角度：120度","个",50]
[7,"五孔插座","250V.10A安全型","个",600]
[8,"双孔网络插座",null,"个",390]
[9,"白面板",null,"个",200]
[10,"软灯带","8*16硅胶灯带、4200K、","米",400]
[11,"灯带接头",null,"个",50]
[12,"三开","250V.10A安全型","个",100]
[13,"二开","250V.10A安全型","个",200]
[14,"单开","250V.10A安全型","个",300]
[15,"空调插座","250V.16A安全型","个",200]
[16,"安全出口指示牌",null,"个",40]
[17,"吊装疏散指示牌",null,"个",20]
[18,"向左疏散指示牌",null,"个",40]
[19,"向右疏散指示牌",null,"个",40]
["报价单位名称（盖公章）：",{"$nulls":4},"法定代表人或授权委托人及联系方式（名字+电话）："]
["报价说明：1、报价采用固定综合单价，报价包含材料费、运输费、上下车费、管理费、利润、税金、风险以及乙方因出售该物资应缴纳的一切税费等全部费用，在整个供货期内均不调整单价，具体金额以实际结算金额为准"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}