{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["C.2 工程项目招标控制价扉页(扉-2)","D 工程项目计价总说明(表-01)","F.1.1 分部分项工程和单价措施项目清单与计价表(表-08~"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"C.2 工程项目招标控制价扉页(扉-2)","index":0,"n_rows":13,"n_cols":23,"rows_kept":13,"merged":[[0,0,0,4],[0,5,0,19],[0,20,0,22],[1,0,1,22],[2,0,2,5],[2,6,2,21],[3,0,4,5],[3,6,4,20],[3,21,4,22],[5,0,5,2],[5,3,5,6],[5,7,5,13],[5,14,5,17],[5,18,5,22],[6,1,6,7],[6,8,6,14],[6,15,6,22],[7,0,7,1],[7,2,7,8],[7,9,7,12],[7,13,7,16],[7,17,7,22],[8,0,8,2],[8,3,8,8],[8,9,8,15],[8,16,8,22],[9,0,9,1],[9,2,9,7],[9,8,9,11],[9,12,9,16],[9,17,9,22],[10,1,10,9],[10,10,10,15],[10,16,10,22],[11,0,11,3],[11,4,11,10],[11,11,11,18],[11,19,11,22],[12,0,12,22]],"flags":["formulas_cached_only"]}
["","","","","","康馨园新增围墙（220米）、地面、绿化工程","","","","","","","","","","","","","","","工程","",""]
["招 标 控 制 价","","","","","","","","","","","","","","","","","","","","","",""]
["招标控制价(小写):","","","","","","394101.37元","","","","","","","","","","","","","","","",""]
["(大写):","","","","","","叁拾玖万肆仟壹佰零壹元叁角柒分","","","","","","","","","","","","","","","",""]
["","","","","","","","","","","","","","","","","","","","","","",""]
["招　标　人:","",""," ","","","","","","","","","","","造价咨询人:","","",""," ","","","",""]
["","(单位盖章)","","","","","","","","","","","","","","(单位资质专用章)","","","","","","",""]
["法定代表人\r\n或其授权人:",""," ","","","","","","","","","","","法定代表人\r\n或其授权人:","","",""," ","","","","",""]
["       ","","","(签字或盖章)","","","","","","","","","","","","","(签字或盖章)","","","","","",""]
["编　制　人:",""," ","","","","","","","","","","复　核　人:","","","",""," ","","","","",""]
["","(造价人员签字盖专用章)","","","","","","","","","","","","","","","(造价工程师签字盖专用章)","","","","","",""]
["编 制 时 间:","","",""," ","","","","","","","复 核 时 间:","","","","","","",""," ","","",""]
["扉-2    ","","","","","","","","","","","","","","","","","","","","","",""]

{"sheet":"D 工程项目计价总说明(表-01)","index":1,"n_rows":3,"n_cols":3,"rows_kept":3,"merged":[[0,0,0,2],[2,0,2,2]],"flags":["formulas_cached_only"]}
["总   说   明","",""]
["工程名称：","康馨园新增围墙（220米）、地面、绿化工程",""]
["1.环境保护、文明施工、安全施工、临时设施等费用应包含在综合单价中，结算时不再单独计取。\r\n2.投标人应向招标人提供增值税发票。\r\n3.税金不作为竞争项目（评审价格为不含税总价）。\r\n4.工程量为预算工程量，结算时按实际发生工程量计取，工程量变化投标单价均不调整。\r\n5.工程量计算按2015年 《四川省建设工程工程量清单计价定额》计算规则计取。\r\n6.投标人投标单价上下浮不得超过招标单价的25%。","",""]

{"sheet":"F.1.1 分部分项工程和单价措施项目清单与计价表(表-08~","index":2,"n_rows":37,"n_cols":12,"rows_kept":37,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,7],[1,8,1,10],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,8],[2,9,2,11],[3,7,4,8],[3,9,4,9],[3,10,4,11],[5,1,5,2],[5,7,5,8],[5,10,5,11],[6,1,6,2],[6,7,6,8],[6,10,6,11],[7,1,7,2],[7,7,7,8],[7,10,7,11],[8,1,8,2],[8,7,8,8],[8,10,8,11],[9,1,9,2],[9,7,9,8],[9,10,9,11],[10,1,10,2],[10,7,10,8],[10,10,10,11],[11,1,11,2],[11,7,11,8],[11,10,11,11],[12,1,12,2],[12,7,12,8],[12,10,12,11],[13,1,13,2],[13,7,13,8],[13,10,13,11],[14,1,14,2],[14,7,14,8],[14,10,14,11],[15,1,15,2],[15,7,15,8],[15,10,15,11],[16,1,16,2],[16,7,16,8],[16,10,16,11],[17,1,17,2],[17,7,17,8],[17,10,17,11],[18,1,18,2],[18,7,18,8],[18,10,18,11],[19,1,19,2],[19,7,19,8],[19,10,19,11],[20,1,20,2],[20,7,20,8],[20,10,20,11],[21,1,21,2],[21,7,21,8],[21,10,21,11],[22,1,22,2],[22,7,22,8],[22,10,22,11],[23,1,23,2],[23,7,23,8],[23,10,23,11],[24,1,24,2],[24,7,24,8],[24,10,24,11],[25,1,25,2],[25,7,25,8],[25,10,25,11],[26,1,26,2],[26,7,26,8],[26,10,26,11],[27,1,27,2],[27,7,27,8],[27,10,27,11],[28,1,28,2],[28,7,28,8],[28,10,28,11],[29,1,29,2],[29,7,29,8],[29,10,29,11],[30,1,30,2],[30,7,30,8],[30,10,30,11],[31,1,31,2],[31,7,31,8],[31,10,31,11],[32,1,32,2],[32,7,32,8],[32,10,32,11],[33,1,33,2],[33,7,33,8],[33,10,33,11],[34,0,34,9],[34,10,34,11],[35,0,35,9],[35,10,35,11],[36,0,36,9],[36,10,36,11]],"flags":["formulas_cached_only"]}
["分部分项工程招标清单","","","","","","","","","","",""]
["工程名称：","","康馨园新增围墙（220米）、地面、绿化工程\\单项工程1【建筑与装饰工程】","","","","","","标段：","","",""]
["序号","项目编码","","项目名称","项目特征","计量\r\n单位","工程\r\n量","招标价格（元）","","投标单价（元）\r\n","",""]
["","","","","","","","招标单价","","投标单价（不含税）","合价（不含税）",""]
["","","","","","","","","","","",""]
["1","010101003015","","人工沟槽土方","1.土壤类别：综合\r\n2.挖土深度：深2m以内","m3","207.68","20.83","","",null,""]
["2","010103001016","","回填方","1.土质要求：一般土壤\r\n2.密实度要求：按规范要求，夯填\r\n3.运距：投标人自行考虑","m3","103.136","11.07","","",null,""]
["3","010103002017","","余方弃置","1.土质要求：一般土壤\r\n2.密实度要求：按规范要求，夯填\r\n3.运距：投标人自行考虑","m3","104.544","9.41","","",null,""]
["4","010501001018","","C15商品砼垫层","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C15\r\n3.泵送费用包含在综合单价中","m3","22","501.78","","",null,""]
["5","010501002019","","带形基础","1.混凝土种类：商品砼\r\n2.混凝土强度等级：C25\r\n3.泵送费用包含在综合单价中","m3","44","521.50","","",null,""]
["6","010515001020","","现浇构件钢筋","1.钢筋种类、规格:II级、螺纹钢（规格综合考虑）","t","0.826","5687.38","","",null,""]
["7","010401009005","","实心砖柱","1.M7.5水泥砂浆砖柱\r\n","m3","21.028","583.71","","",null,""]
["8","010401003001","","实心砖墙","1.M7.5水泥砂浆砖围墙\r\n2.挡土墙上砌筑，无基础","m3","33.044","585.26","","",null,""]
["9","011204003002","","矮墙贴外墙纸皮砖","1.13mm厚水泥砂浆打底\r\n2.粘结剂贴外墙纸皮砖","m2","319.521","128.97","","",null,""]
["10","010507007006","","C25混凝土压顶","1.C25混凝土压顶\r\n2.泵送费用包含在综合单价中","m3","7.079","540.91","","",null,""]
["11","011205002003","","砖柱贴外墙纸皮砖","1.13mm厚水泥砂浆打底\r\n2.粘结剂贴外墙纸皮砖","m2","224.256","136.74","","",null,""]
["12","010607002004","","成品栅栏","1.材料品种、规格：钢矩管，规格详见设计(栏杆单价参凉山州信息扁铁栏杆)\r\n2.刷两道防锈漆，两道氟碳漆","m2","330.871","154.52","","",null,""]
["13","040202001007","","路床（槽）整形","路床（槽）整形","m2","500","1.61","","",null,""]
["14","040202006008","","建渣回填路面、碾压","建渣回填路面、碾压300mm厚","m2","500","33.76","","",null,""]
["15","040202015009","","水泥稳定碎（砾）石","1.水泥稳定砂砾基层（水泥含量） 5% 压实厚度(cm) 20","m2","500","56.57","","",null,""]
["16","040203006010","","沥青混凝土路面","1.喷透层油 \r\n2.中粒式沥青混凝土60mm厚 \r\n3.细粒式沥青混凝土40mm厚 \r\n","m2","500","122.10","","",null,""]
["17","010501001013","","花池砖下C10混凝土垫层","花池砖下C10混凝土垫层","m3","2","491.68","","",null,""]
["18","010401012011","","花池零星砌砖","花池零星砌砖","m3","3.6","615.78","","",null,""]
["19","011203001012","","花池零星抹灰","花池零星抹灰","m2","32","51.62","","",null,""]
["20","011206002014","","花池贴纸皮砖","花池贴纸皮砖","m2","27","112.46","","",null,""]
["21","050102001005","","腊梅 Φ10","1.种类：腊梅\r\n2.米径：Φ10cm\r\n3.树高、冠幅：树高1.5~2.5m、冠幅2~2.5m\r\n4.分枝点：0.6m\r\n5.养护期：2年，成活及保存养护的费用综合考虑在报价中，满足设计及规范要求\r\n6.树型要求：带土球,全冠,主干通直,树形优美,植株健壮\r\n7.草绳所绕树干高度：综合考虑，且满足设计及规范要求\r\n8.树木支撑材料数量：综合考虑，满足设计及相关规范要求\r\n9.其他:满足设计、技术规范、施工验收规范及招标文件要求","株","4","1678.53","","",null,""]
["22","050101009001","","种植土回（换）填","1.回填土质要求：种植土满足规范要求\r\n2.取土运距：综合考虑\r\n3.回填厚度：综合考虑\r\n4.本项目包括种植土造坡，费用综合考虑在报价中\r\n5.其他：满足设计及规范要求","m3","90","34.68","","",null,""]
["23","050101010001","","整理绿化用地","1.整地要求:清除杂草、清理土壤表面的石块等杂物并外运、20cm以内土壤嵌细（土壤颗粒小于2cm）、找平、造坡达到规范要求\r\n2.土质要求:满足种植要求\r\n3.取土运距:综合考虑\r\n4.挖填厚度:综合考虑","m2","300","4.61","","",null,""]
["24","050102008001","","海桐球","1.苗木、花卉种类 ：海桐球\r\n2.冠高或蓬径：高度0.8m、冠幅0.8~1m\r\n3.养护期:2年，成活及保存养护的费用综合考虑在报价中，满足设计及规范要求\r\n4.已养护修剪成球形,姿态饱满,植株健壮\r\n5.其他:满足设计、技术规范、施工验收规范及招标文件要求","m2","30","117.35","","",null,""]
["25","050102012001","","草坪","1.草皮种类：草坪 \r\n2.铺种方式：满铺，密不见土\r\n3.养护期：2年，成活及保存养护的费用综合考虑在报价中，满足设计及规范要求","m2","270","59.00","","",null,""]
["26","011701003008","","里脚手架","1．搭设方式 \r\n2．搭设高度 \r\n3．脚手架材质","m2","245.76","7.08","","",null,""]
["27","011702025007","","压顶模板","压顶模板","m","194.63","43.76","","",null,""]
["28","011706001001","","技工"," ","个","5","280.00","","",null,""]
["29","011706002001","","普工","1.机械规格型号 \r\n2.降排水管规格","个","5","150.00","","",null,""]
["不含税总价",{"$nulls":10},""]
["税率",{"$nulls":10},""]
["含税总价",{"$nulls":10},""]