{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":9,"rows_kept":6,"merged":[[0,0,0,8],[4,0,4,7],[5,0,5,1],[5,3,5,5],[5,6,5,8]]}
["雅安市新型冠状病毒肺炎集中收治方舱医院改建工程项目电梯工程采购"]
["序号","项目名称","项目特征描述","计量\r\n单位","数量","设备价格（含税）","安装费用（含税）","运输费（含税）","合计"]
[1,"客梯（患者电梯兼无障碍电梯）","1.名称：客梯（患者电梯兼无障碍电梯） \r\n2.型号：DT1，载重1600kg ，无机房电梯\r\n3.用途：载人 \r\n4.层数：1F-3F \r\n5.站数：3站 \r\n6.提升高度、速度：高度：结构高度13.4m，提升速度1m/s，冲顶高度为4500mm\r\n7.配线材质、规格、敷设方式：按设计 \r\n8.运转调试要求：含调试、运转等全部费用及手续","部","1"]
[2,"货梯（污物电梯）","1.名称：货梯（污物电梯） \r\n2.型号：DT2，载重1600kg ，无机房电梯\r\n3.用途：载人 \r\n4.层数：1F-3F \r\n5.站数：3站 \r\n6.提升高度、速度：高度：结构高度13.4m，提升速度1m/s，冲顶高度为4500mm\r\n7.配线材质、规格、敷设方式：按设计 \r\n8.运转调试要求：含调试、运转","部","1"]
["总计（设备税率：13%，安装税率：3%）："]
["供应商（盖章）：",null,null,"联系方式："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}