{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["C.2 工程项目招标控制价扉页(扉-2)","F.1.1 分部分项工程清单计价表(表-08)【消防安装工程】"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"C.2 工程项目招标控制价扉页(扉-2)","index":0,"n_rows":13,"n_cols":23,"rows_kept":13,"merged":[[0,0,0,4],[0,5,0,19],[0,20,0,22],[1,0,1,22],[2,0,2,5],[2,6,2,21],[3,0,4,5],[3,6,4,20],[3,21,4,22],[4,0,4,5],[4,6,4,20],[4,21,4,22],[5,0,5,2],[5,3,5,6],[5,7,5,13],[5,14,5,17],[5,18,5,22],[6,1,6,7],[6,8,6,14],[6,15,6,22],[7,0,7,1],[7,2,7,8],[7,9,7,12],[7,13,7,16],[7,17,7,22],[8,0,8,2],[8,3,8,8],[8,9,8,15],[8,16,8,22],[9,0,9,1],[9,2,9,7],[9,8,9,11],[9,12,9,16],[9,17,9,22],[10,1,10,9],[10,10,10,15],[10,16,10,22],[11,0,11,3],[11,4,11,10],[11,11,11,18],[11,19,11,22],[12,0,12,22]],"flags":["formulas_cached_only"]}
["","","","","","雅安市新型冠状病毒肺炎集中收治方舱医院改建工程","","","","","","","","","","","","","","","工程","",""]
["招 标 控 制 价","","","","","","","","","","","","","","","","","","","","","",""]
["招标控制价(小写):","","","","","","元","","","","","","","","","","","","","","","",""]
["(大写):","","","","",""," ","","","","","","","","","","","","","","","",""]
["","","","","","","","","","","","","","","","","","","","","","",""]
["招　标　人:","","","四川黎明工程咨询管理有限公司","","","","","","","","","","","造价咨询人:","","","","中天新合建设咨询有限公司","","","",""]
["","(单位盖章)","","","","","","","","","","","","","","(单位资质专用章)","","","","","","",""]
["法定代表人\r\n或其授权人:",""," ","","","","","","","","","","","法定代表人\r\n或其授权人:","","",""," ","","","","",""]
["       ","","","(签字或盖章)","","","","","","","","","","","","","(签字或盖章)","","","","","",""]
["编　制　人:",""," ","","","","","","","","","","复　核　人:","","","",""," ","","","","",""]
["","(造价人员签字盖专用章)","","","","","","","","","","","","","","","(造价工程师签字盖专用章)","","","","","",""]
["编 制 时 间:","","",""," ","","","","","","","复 核 时 间:","","","","","","",""," ","","",""]
["扉-2    ","","","","","","","","","","","","","","","","","","","","","",""]

{"sheet":"F.1.1 分部分项工程清单计价表(表-08)【消防安装工程】","index":1,"n_rows":74,"n_cols":9,"rows_kept":74,"merged":[[0,0,0,8],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,5],[1,6,1,8],[2,6,3,6],[2,7,3,8],[3,4,3,5],[3,7,3,8],[4,4,4,5],[4,7,4,8],[5,4,5,5],[5,7,5,8],[6,4,6,5],[6,7,6,8],[7,4,7,5],[7,7,7,8],[8,4,8,5],[8,7,8,8],[9,4,9,5],[9,7,9,8],[10,4,10,5],[10,7,10,8],[11,4,11,5],[11,7,11,8],[12,4,12,5],[12,7,12,8],[13,4,13,5],[13,7,13,8],[14,4,14,5],[14,7,14,8],[15,4,15,5],[15,7,15,8],[16,4,16,5],[16,7,16,8],[17,4,17,5],[17,7,17,8],[18,4,18,5],[18,7,18,8],[19,4,19,5],[19,7,19,8],[20,4,20,5],[20,7,20,8],[21,4,21,5],[21,7,21,8],[22,4,22,5],[22,7,22,8],[23,4,23,5],[23,7,23,8],[24,4,24,5],[24,7,24,8],[25,4,25,5],[25,7,25,8],[26,4,26,5],[26,7,26,8],[27,4,27,5],[27,7,27,8],[28,4,28,5],[28,7,28,8],[29,4,29,5],[29,7,29,8],[30,4,30,5],[30,7,30,8],[31,4,31,5],[31,7,31,8],[32,4,32,5],[32,7,32,8],[33,4,33,5],[33,7,33,8],[34,4,34,5],[34,7,34,8],[35,4,35,5],[35,7,35,8],[36,4,36,5],[36,7,36,8],[37,4,37,5],[37,7,37,8],[38,4,38,5],[38,7,38,8],[39,4,39,5],[39,7,39,8],[40,4,40,5],[40,7,40,8],[41,4,41,5],[41,7,41,8],[42,4,42,5],[42,7,42,8],[43,4,43,5],[43,7,43,8],[44,4,44,5],[44,7,44,8],[45,4,45,5],[45,7,45,8],[46,4,46,5],[46,7,46,8],[47,4,47,5],[47,7,47,8],[48,4,48,5],[48,7,48,8],[49,4,49,5],[49,7,49,8],[50,4,50,5],[50,7,50,8],[51,4,51,5],[51,7,51,8],[52,4,52,5],[52,7,52,8],[53,4,53,5],[53,7,53,8],[54,4,54,5],[54,7,54,8],[55,4,55,5],[55,7,55,8],[56,4,56,5],[56,7,56,8],[57,4,57,5],[57,7,57,8],[58,4,58,5],[58,7,58,8],[59,4,59,5],[59,7,59,8],[60,4,60,5],[60,7,60,8],[61,4,61,5],[61,7,61,8],[62,4,62,5],[62,7,62,8],[63,4,63,5],[63,7,63,8],[64,4,64,5],[64,7,64,8],[65,4,65,5],[65,7,65,8],[66,4,66,5],[66,7,66,8],[67,4,67,5],[67,7,67,8],[68,4,68,5],[68,7,68,8],[69,4,69,5],[69,7,69,8],[70,0,70,6],[70,7,70,8],[71,0,71,6],[72,0,72,6],[72,7,72,8],[73,0,73,1],[73,2,73,3],[73,4,73,7]],"flags":["formulas_cached_only"]}
["雅安市新型冠状病毒肺炎集中收治方舱医院改建工程项目消防安装工程"]
["序号","项目名称","项目特征描述","计量\r\n单位","工程量","","金额（元）","",""]
["","","","","","","不含税单价","不含税单价合计",""]
["","","","","","","","",""]
[" ","新建部分"," "," "," ",""," "," ",""]
["1","水喷淋镀锌钢管 DN25","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","299.55",""," ","",""]
["2","水喷淋镀锌钢管 DN32","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","136.75",""," ","",""]
["3","水喷淋镀锌钢管 DN40","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","76.33",""," ","",""]
["4","水喷淋镀锌钢管 DN50","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","42.3",""," ","",""]
["5","水喷淋镀锌钢管 DN65","1.安装部位 \n2.材质、规格 \n3.连接形式 \n4. 钢管镀锌设计要求 \n5.压力试验及冲洗设计要求 \n6.管道标识设计要求","m","13.7",""," ","",""]
["6","水喷淋镀锌钢管 DN80","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","66.55",""," ","",""]
["7","水喷淋镀锌钢管 DN100","1.安装部位 \r\n2.材质、规格 \r\n3.连接形式 \r\n4. 钢管镀锌设计要求 \r\n5.压力试验及冲洗设计要求 \r\n6.管道标识设计要求","m","61.5",""," ","",""]
["8","自喷喷头 ZST15","1.安装部位 \r\n2.材质、型号、规格 \r\n3.连接形式 \r\n4.装饰盘设计要求","个","163",""," ","",""]
["9","管道支架","1.材质 \r\n2.管架形式","Kg","302.98",""," ","",""]
["10","加厚热浸镀锌喷淋管 DN25","1.名称：加厚热浸镀锌喷淋管\n2.介质：综合考虑\n3.规格：DN25\n4.管道压力等级，综合考虑\n5.管道镀锌方式（热镀锌、热浸镀锌）综合考虑\n6.连接形式：螺纹连接\n7.管道敷设部位及方式：综合考虑\n8.含管道及各类管件制作、安装、管道标识\n9.含水压试验、管道冲洗综合考虑\n10.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","44.23",""," ","",""]
["11","加厚热浸镀锌喷淋管 DN50","1.名称：加厚热浸镀锌喷淋管\n2.介质：综合考虑\n3.规格：DN50\n4.管道压力等级，综合考虑\n5.管道镀锌方式（热镀锌、热浸镀锌）综合考虑\n6.连接形式：螺纹连接\n7.管道敷设部位及方式：综合考虑\n8.含管道及各类管件制作、安装、管道标识\n9.含水压试验、管道冲洗综合考虑\n10.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","146.63",""," ","",""]
["12","加厚热浸镀锌喷淋管 DN65","1.名称：加厚热浸镀锌喷淋管\r\n2.介质：综合考虑\r\n3.规格：DN65\r\n4.管道压力等级，综合考虑\r\n5.管道镀锌方式（热镀锌、热浸镀锌）综合考虑\r\n6.连接形式：沟槽式卡箍连接\r\n7.管道敷设部位及方式：综合考虑\r\n8.含管道及各类管件制作、安装、管道标识\r\n9.含水压试验、管道冲洗综合考虑\r\n10.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","71.43",""," ","",""]
["13","加厚热浸镀锌喷淋管 DN100","1.名称：加厚热浸镀锌喷淋管\n2.介质：综合考虑\n3.规格：DN100\n4.管道压力等级，综合考虑\n5.管道镀锌方式（热镀锌、热浸镀锌）综合考虑\n6.连接形式：沟槽式卡箍连接\n7.管道敷设部位及方式：综合考虑\n8.含管道及各类管件制作、安装、管道标识\n9.含水压试验、管道冲洗综合考虑\n10.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","134.97",""," ","",""]
["14","手提式磷酸铵盐灭火器 MF/ABC5（带箱）","1.安装部位及方式：综合考虑 \r\n2.型号、规格：单栓、DN65 \r\n3.箱体规格、材质、表面处理工艺及颜色综合考虑\r\n4.箱内配置综合考虑，含灭火器\r\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","套","145",""," ","",""]
["15","带自救式消防卷盘的组合式消防柜","1.名称：室内消火栓\n2.型号：带自救式消防卷盘的组合式消防柜（内设灭火器）\n3.规格：详设计\n4.附件配置：消火栓箱内衬胶龙带（25m）、铝合金水枪（QZ19/19）、消防卷盘（JPS1.0-19）和软管（25m）等成套配置\n5.安装方式：明装\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","套","9",""," ","",""]
["16","单栓口消火栓箱SG18E65Z-J ","1.名称：单栓口消火栓箱 \r\n2.型号：SG18E65Z-J\r\n3.规格：箱体尺寸 1.8×0.7×0.18\r\n4.附件配置：消火栓箱内衬胶龙带、铝合金水枪、消防卷盘和软管等成套配置\r\n5.安装方式：明装\r\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","套","10",""," ","",""]
["17","水灭火控制装置调试","自动喷水灭火系统","点","4",""," ","",""]
[" ","改造部分"," "," "," ",""," "," ",""]
["18","拆除消火栓管 DN65","1.安装部位(室内、外):室内,拆除消火栓管 DN65\r\n2.材质：镀锌钢管\r\n3.规格：DN65\r\n4.连接方式：卡箍连接","m","48",""," ","",""]
["19","拆除消火栓管 DN100","1.安装部位(室内、外):室内,拆除消火栓管 DN100\n2.材质：镀锌钢管\n3.规格：DN100\n4.连接方式：卡箍连接","m","24",""," ","",""]
["20","拆除蝶阀 DN65","1.名称：蝶阀\r\n2.规格型号：DN65\r\n7.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","15",""," ","",""]
["21","拆除消防柜","1.名称：拆除原有消防柜\r\n2.规格、 型号：按原有","套","15",""," ","",""]
["22","安装消火栓管（利旧） DN65","1.安装部位(室内、外):室内\r\n2.材质：镀锌钢管\r\n3.规格：DN65\r\n4.连接方式：卡箍连接","m","48",""," ","",""]
["23","安装消火栓管（利旧） DN100","1.安装部位(室内、外):室内\r\n2.材质：镀锌钢管\r\n3.规格：DN65\r\n4.连接方式：卡箍连接","m","24",""," ","",""]
["24","安装蝶阀（利旧）DN65","1.名称：安装蝶阀（利旧）\r\n2.材质：详设计\r\n3.型号、规格：DN65\r\n4.连接形式：法兰连接\r\n5.安装部位：详设计\r\n6.包含制垫、加垫、阀门连接、紧螺栓、水压试验、法兰片\r\n7.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","15",""," ","",""]
["25","安装消防柜（利旧）","1.名称：安装消防柜（利旧）\r\n2.规格、 型号：按原有","套","15",""," ","",""]
["26","铸铁蝶阀 SJKD-16Q DN50","1.类型：铸铁蝶阀 \r\n2.材质：铸铁\r\n3.型号、规格：SJKD-16Q DN50","个","4",""," ","",""]
["27","铸铁蝶阀 SJKD-16Q DN65","1.类型：铸铁蝶阀 \r\n2.材质：铸铁\r\n3.型号、规格：SJKD-16Q DN65","个","3",""," ","",""]
["28","铸铁蝶阀 SJKD-16Q DN100","1.类型：铸铁蝶阀 \r\n2.材质：铸铁\r\n3.型号、规格：SJKD-16Q DN100","个","9",""," ","",""]
["29","阻火圈 DN100","1.材质：钢质 \r\n2.结构形式：卡箍\r\n3.型号、规格：DN100 ","个","6",""," ","",""]
[" ","应急照明系统"," "," "," ",""," "," ",""]
["30","单向疏散指示灯（自带蓄电池）","1.名称：单向疏散指示灯（自带蓄电池） \r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","16",""," ","",""]
["31","双向疏散指示灯（自带蓄电池）","1.名称：双向疏散指示灯（自带蓄电池）\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","18",""," ","",""]
["32","复合疏散指示标志灯","1.名称：复合疏散指示标志灯\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","5",""," ","",""]
["33","顶装式（或顶嵌式）应急灯","1.名称：顶装式（或顶嵌式）应急灯\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","94",""," ","",""]
["34","安全出口指示灯","1.名称：安全出口指示灯\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","12",""," ","",""]
["35","双头顶装式（或顶嵌式）应急灯","1.名称：双头顶装式（或顶嵌式）应急灯\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","9",""," ","",""]
["36","安全出口标志灯","1.名称：安全出口标志灯\r\n2.型号、规格：详设计 \r\n3.安装方式：详设计","套","10",""," ","",""]
[" ","消防联动报警系统"," "," "," ",""," "," ",""]
["37","单输入输出模块 TX3208A型","1.名称：双输入/双输出模块\r\n2.型号、规格：具体详设计，自行综合考虑\r\n3.安装方式：模块箱内或控制设备旁安装\r\n4.其他：满足设计及规范要求","只","44",""," ","",""]
["38","消防断电模块","1.名称：消防断电模块\r\n2.型号、规格：具体详设计，自行综合考虑\r\n3.安装方式：详设计\r\n4.其他：满足设计及规范要求","个","4",""," ","",""]
["39","消防模块箱","1.名称：消防模块箱\r\n2.型号、规格：具体详设计，自行综合考虑\r\n3.安装方式：底距地2.4m明装\r\n4.配套设备：含箱体及箱内成套元器配件安装\r\n5.其他：满足设计及规范要求","个","3",""," ","",""]
["40","4门控制器","1.名称：4门控制器（不含蓄电池）\r\n2.规格：管控门数4门、存储容量10万张卡和30万记录存储、支持蓄电池（303700655 OT7-12蓄电池）接入\r\n3.机箱尺寸：345mmx370mmx90mm\r\n4.工作电压：自带机箱和供电电源（AC220V输入），工作电压DC 12V,功耗≤4W（不带负载）","台","11",""," ","",""]
["41","扬声器 3W","1.名称：广播扬声器（吸顶/壁挂综合考虑）\n2.型号、规格：具体详设计，自行综合考虑\n3.安装方式：底边距地2.3m安装\n4.附件配置：含底座安装\n5.安装位置：扬声器设置在走道和大厅等公共场所。每个扬声器的功率不小于3W，其数量保证从一个防火分区内的任何部位到最近一个扬声器的直线距离不大于25m，走道末端距最近的扬声器距离不大于12.5m。\n5.其他：满足设计及规范要求","只","33",""," ","",""]
["42","镀锌钢管 SC20","1.名称：穿钢管 SC20\r\n2.材质：镀锌钢管\r\n3.规格：SC20\r\n4.配置形式及部位：砖、混凝土结构暗配","m","86.83",""," ","",""]
["43","紧定钢管 JDG20","1.名称：紧定钢管 JDG20\r\n2.材质：紧定钢管\r\n3.规格：JDG20\r\n4.配置形式及部位：砖、混凝土结构明配","m","400.14",""," ","",""]
["44","紧定钢管 JDG25","1.名称：紧定钢管 JDG25\n2.材质：紧定钢管\n3.规格：JDG25\n4.配置形式及部位：砖、混凝土结构明配","m","114.99",""," ","",""]
["45","多芯屏蔽线 NH-RVVP-2×1.5","1.名称：多芯屏蔽线 NH-RVVP-2×1.5\r\n2.型号、规格：NH-RVVP-2×1.5\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","26.96",""," ","",""]
["46","耐火双绞屏蔽线 NH-RVSP-4×1.0","1.名称：耐火双绞屏蔽线 NH-RVSP-4×1.0\r\n2.型号、规格：NH-RVSP-4×1.0\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","106.83",""," ","",""]
["47","耐火双绞线 NH-RVS-2*1.5mm2","1.名称：耐火双绞线 NH-RVS-2*1.5mm2\r\n2.型号、规格：NH-RVS-2*1.5mm2\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","169.46",""," ","",""]
["48","耐火铜芯软线 NH-BVR-2×","1.名称：耐火铜芯软线 NH-BVR-2×2.5\n2.型号、规格：NH-BVR-2×2.5\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\n4.其他：满足设计及规范要求","m","184.18",""," ","",""]
["49","阻燃铜芯电源线 ZR-BVR-2×1.5","1.名称：阻燃铜芯电源线 ZR-BVR-2×1.5\r\n2.型号、规格：ZR-BVR-2×1.5\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","369.52",""," ","",""]
["50","自动报警系统调试","自动报警系统调试","系统","1",""," ","",""]
[" ","火灾自动报警系统"," "," "," ",""," "," ",""]
["51","声光报警器 TX3301型","1.名称：火灾声光警报器\r\n2.型号、规格：TX3301型\r\n3.安装方式：底距地2.3m明装\r\n4.附件配置：含底座安装\r\n5.其他：满足设计及规范要求","只","25",""," ","",""]
["52","总线隔离模块 TX3219型","1.名称：总线隔离器\n2.型号、规格：TX3219型\n3.安装方式：安装于接线端子箱内或根据现场实际情况确定\n4.若吸顶安装含底座盒\n5.其他：满足设计及规范要求","只","8",""," ","",""]
["53","感烟探测器（TX3100A型）","1.名称：感烟探测器\r\n2.型号、规格：TX3100A型\r\n3.安装方式：吸顶安装\r\n4.附件配置：含底座安装\r\n5.其他：满足设计及规范要求","只","57",""," ","",""]
["54","手动报警按钮（带消防电话插孔） TX3140型","1.名称：带电话插孔的手动报警按钮\r\n2.型号、规格：TX3140型\r\n3.安装方式：底距地1.5m明装\r\n4.附件配置：含底座安装\r\n5.其他：满足设计及规范要求","只","12",""," ","",""]
["55","消火栓按钮 TX3152型","1.名称：消火栓报警按钮\r\n2.型号、规格：具体详设计，自行综合考虑\r\n3.安装方式：底距地1.5m，消火栓箱内安装或根据现场实际需要位置及高度进行安装\r\n4.附件配置：含底座安装\r\n5.其他：满足设计及规范要求","只","8",""," ","",""]
["56","紧定钢管 JDG20","1.名称：紧定钢管 JDG20\r\n2.材质：紧定钢管\r\n3.规格：JDG20\r\n4.配置形式及部位： 砖、混凝土结构明配","m","541.92",""," ","",""]
["57","紧定钢管 JDG25","1.名称：紧定钢管 JDG25\r\n2.材质：紧定钢管\r\n3.规格：JDG25\r\n4.配置形式及部位：砖、混凝土结构明配","m","98.45",""," ","",""]
["58","耐火双绞线 NH-RVS-2*1.5","1.名称：电气配线\r\n2.型号、规格：NH-RVS-2*1.5mm2\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","499.9",""," ","",""]
["59","耐火铜芯软线 NH-BVR-2×2.5","1.名称：电气配线\r\n2.型号、规格：ZC-BVR-2*1.5mm2\r\n3.敷设方式：穿管、桥架等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","312.25",""," ","",""]
["60","多芯屏蔽线 NH-RVVP-2×1.5","1.名称：控制电缆\r\n2.型号、规格：NH-KVV-2*1.5mm2\r\n3.敷设方式：穿管、桥架（含井道）等敷设，综合考虑，双色线价差综合考虑\r\n4.其他：满足设计及规范要求","m","343.23",""," ","",""]
["61","自动报警系统调试","自动报警系统调试","系统","1",""," ","",""]
["不含税价合计：",{"$nulls":6},""]
["税金（税率9%）："]
["含税价合计：",{"$nulls":6},""]
["供应商（盖章）：",{"$nulls":3},"联系方式："]