{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["沥青混凝土路面"],"read":"whole","date_system":"1900"}

{"sheet":"沥青混凝土路面","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"merged":[[0,0,0,7],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,1],[27,2,27,4],[27,5,27,7],[28,0,28,7]]}
["蒙顶壹号项目公区和地下室灯具报价表"]
["序号","材料名称","材质/规格型号","单位","暂定工程量","不含税单价（元）","不含税合计（元）","备注"]
[1,"吊线LED灯盘","(色温4000k,28W)1200*65*40","套",71,null,null,"国产一线品牌"]
[2,"吊线LED灯盘","(色温4000k,42W)1500*100*50","套",8,null,null,"国产一线品牌"]
[3,"LED斗胆灯","(色温3000k,2*3W)","套",65,null,null,"国产一线品牌"]
[4,"LED筒灯","(色温3000k,3W)","套",497,null,null,"国产一线品牌"]
[5,"LED筒灯","(色温3000k,12W)","套",1085,null,null,"国产一线品牌"]
[6,"暗装单联单控翘板开关",null,"只",24,null,null,"国产一线品牌"]
[7,"暗装三联单控翘板开关",null,"只",13,null,null,"国产一线品牌"]
[8,"暗装双联单控翘板开关",null,"只",24,null,null,"国产一线品牌"]
[9,"成品定制灯盘","(色温4000k,36W)","套",10,null,null,"国产一线品牌"]
[10,"灯带","（色温3000k,4.5W/m）","m",174,null,null,"国产一线品牌"]
[11,"普通二、三极安全插座",null,"套",17,null,null,"国产一线品牌"]
[12,"声光感应延时开关",null,"个",557,null,null,"国产一线品牌"]
[13,"吸顶灯","(色温4000k,18W)","套",37,null,null,"国产一线品牌"]
[14,"吸顶式射灯","(色温4000k,7W)","套",56,null,null,"国产一线品牌"]
[15,"带反射罩灯，壁挂式灯长条灯","LED,18W","套",91,null,null,"国产一线品牌"]
[16,"带反射罩灯，壁挂式灯长条灯，带感应开关","LED,18W","套",5,null,null,"国产一线品牌"]
[17,"带反射罩灯,单管长条形","LED,18W","套",822,null,null,"国产一线品牌"]
[18,"带反射罩灯,双管长条形","LED,2x14W","套",47,null,null,"国产一线品牌"]
[19,"灯具吊杆","φ15","根",1850,null,null,"国产一线品牌"]
[20,"防水防尘灯单管荧光灯","LED,18W","套",37,null,null,"国产一线品牌"]
[21,"井道壁挂式灯座,长条形","LED,10W","套",34,null,null,"国产一线品牌"]
[22,"吸顶灯,自带感应开关","LED,18W","套",23,null,null,"国产一线品牌"]
["不含税总价（元）："]
["税率：",{"$nulls":5},"%"]
["含税总价（元）："]
["供应商名称（盖公章）：",{"$nulls":4}," 联系电话："]
["注：报价包含材料费、人工费、运输费、上下车费、管理费、利润、税费、风险等全部费用，在整个服务期内均不调整材料单价，具体金额以实际结算金额为准。"]