{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":11},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"merged":[[0,0,0,8],[11,0,11,6],[12,0,12,6],[13,0,13,6],[14,0,14,3],[14,5,14,8],[15,0,15,8]]}
["四川省区域应急救援雅安基地项目环氧地坪漆清单"]
["序号","名称","规格型号","单位","数量","不含税控制单价（元）","不含税\n单价（元）","不含税金额（元）","备注"]
[1,"环氧砂浆地坪",".基础类型：细石混凝土找坡层\n2.材料种类：无溶剂环氧地坪\n3.技术参数：厚度1.5mm\n4.涂刷要求：素地处理、底漆一遍、砂浆层、中涂层、腻子层一遍、面漆两遍\n5.施工部位：车库停车区","m²",3034.33,{"v":35,"d":"35.00"},null,{"$f":"E3*G3","v":{"v":0,"d":"0.00"}}]
[2,"超耐磨地坪","1.基础类型：混凝土磨光面\n2.材料种类：聚氨酯耐候地坪\n3.技术参数：厚度1.5mm\n4.涂刷要求：素地处理、底漆一遍、砂浆层、中涂层、腻子层一遍、自流平面漆层一遍、刮涂超耐磨涂层\n5.施工部位：应急物资储备库首层重装架空层","m²",1751.78,{"v":39,"d":"39.00"},null,{"v":0,"d":"0.00"}]
[3,"环氧抛砂防滑斜坡","1.基础类型：混凝土结构板压光\n2.材料种类：环氧抛砂防滑斜坡\n3.技术参数：厚度3.0mm\n4.涂刷要求：素地处理、底漆一遍、砂浆层、中涂层、腻子层一遍、抛砂层、面涂层两遍\n5.施工部位：机动车库坡道、非机动车库坡道","m²",436,{"v":50,"d":"50.00"},null,{"v":0,"d":"0.00"}]
[4,"面层级水泥基自流平","1.基础类型：落差不大于4mm混凝土结构板\n2.材料种类：面层级水泥基自流平\n3.技术参数：厚度8.0mm\n4.涂刷要求：基础地面进行打磨→打磨后扫掉灰尘→界面剂两遍→漫涂自流平\n5.施工部位：倒塌房屋模型训练场","m²",822,{"v":59,"d":"59.00"},null,{"v":0,"d":"0.00"}]
[5,"面层级水泥基自流平","1.基础类型：落差不大于4mm混凝土结构板\n2.材料种类：面层级水泥基自流平\n3.技术参数：厚度8.0mm\n4.涂刷要求：基础地面进行打磨→打磨后扫掉灰尘→界面剂两遍→漫涂自流平\n5.施工部位：犬舍、活动间、犬粮加工储藏","m²",470.5,{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"}]
[6,"面层级水泥基自流平","1.基础类型：落差不大于4mm混凝土结构板\n2.材料种类：面层级水泥基自流平\n3.技术参数：厚度8.0mm\n4.涂刷要求：基础地面进行打磨→打磨后扫掉灰尘→界面剂两遍→漫涂自流平\n5.施工部位：训练塔1-10层","m²",948.1,{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"}]
[7,"面层级水泥基自流平","1.基础类型：落差不大于4mm混凝土结构板\n2.材料种类：面层级水泥基自流平\n3.技术参数：厚度8.0mm\n4.涂刷要求：基础地面进行打磨→打磨后扫掉灰尘→界面剂两遍→漫涂自流平\n5.施工部位：直升机停机库","m²",695.56,{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"}]
[8,"聚氨酯耐候地坪","1.基础类型：混凝土基础压光\n2.材料种类：聚氨酯耐候地坪\n3.技术参数：厚度1.5mm\n4.涂刷要求：素地处理、底漆一遍、砂浆层、中涂层、腻子层一遍、滚涂耐候面层一遍、耐候保护层\n5.施工部位：应急物资储备库首层重装架空层","m²",807.23,{"v":41,"d":"41.00"},null,{"v":0,"d":"0.00"}]
[9,"聚氨酯耐候地坪","1.基础类型：混凝土基础压光\n2.材料种类：聚氨酯耐候地坪\n3.技术参数：厚度1.5mm\n4.涂刷要求：素地处理、底漆一遍、砂浆层、中涂层、腻子层一遍、滚涂耐候面层一遍、耐候保护层\n5.施工部位：特勤站首层重装架空层","m²",2288.2,{"v":41,"d":"41.00"},null,{"v":0,"d":"0.00"}]
["不含税合计（元）",{"$nulls":6},{"$f":"SUM(H3:H11)","v":{"v":0,"d":"0.00"}}]
["税率：",{"$nulls":6},"%"]
["含税合计（元）"]
["报价单位名称（加盖公章）：",{"$nulls":4},"联系人及联系电话："]
["注：报价采用固定综合单价。分包单位根据清单及图纸自主综合考虑报价，报价保留小数点后两位。报价包含但不限于主材费用、辅材费用、耗材费用、损耗费用、运送费、二次搬运费、二次深化设计费用、卸车、人工费用、资料费、管理费、竣工验收费、材料及分包工程验收试验检测费用、安全文明施工费、措施项目费、赶工费用、成品保护费、分包单位人员薪资和意外伤害保险费、工人食宿费用、分包单位合理利润、完工后清洁工作相关费用、不可预见费用等供应商一切直接和间接费用。至工程完工期间出现的人工、材料等费用的上涨，属于分包单位承担的风险范畴，价款均不予调整。具体金额以实际结算金额为准。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}