{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"merged":[[0,0,0,9]]}
["工程名称：宝兴县灵关保障性租赁住房建设项目"]
["序号","项目名称","拟检测数量（组）","检测项目","不含税单价（元）","税率","含税单价（元）","不含税金额（元）","含税金额（元）","备注"]
[1,"水泥",5,"强度、安定性、凝结时间、标准稠度用水量"]
[2,"砂",5,"颗粒级配、表观密度、堆积密度、含泥量、细度模数、含水量、空隙率"]
[3,"石",10,"颗粒级配、表观密度、堆积密度、含泥量、空隙率、压碎值、针片状含量"]
[4,"混凝土配合比",40,"塌落度、水灰比、砂率、配合比"]
[5,"砂浆配合比",16,"稠度、水灰比、配合比"]
[6,"混凝土抗压",200,"抗压强度"]
[7,"砂浆抗压",80,"抗压强度"]
[8,"砖",20,"抗压强度"]
[9,"钢筋",86,"抗拉强度、断后伸长率、屈服强度"]
[10,"钢管",16,"抗拉强度、断后伸长率、屈服强度"]
[11,"镀锌扁钢",2,"抗拉强度、断后伸长率、屈服强度"]
[12,"PPR管",10,"外观、平均外径、壁厚、纵向回缩率、落锤冲击试验、拉伸屈服强度等"]
[13,"波纹管",1,"外观、平均外径、壁厚、纵向回缩率、落锤冲击试验、拉伸屈服强度等"]
[14,"防水卷材",2,"不透水性、耐热度、拉力、断裂拉伸强度、延伸率、撕裂强度、低温弯折性"]
[15,"PVC管",10,"外观、平均外径、壁厚、纵向回缩率、落锤冲击试验、拉伸屈服强度等"]
[16,"电缆",12,"导体电阻、绝缘层厚度、电压试验"]
[17,"开关",4,"防触电保护、绝缘电阻、电气强度、机械强度、灼热丝试验等"]
[18,"电线",6,"防触电保护、绝缘电阻、电气强度、机械强度、灼热丝试验等"]
[19,"插座",4,"防触电保护、绝缘电阻、电气强度、机械强度、灼热丝试验等"]
[20,"窗",1,"传热系数、气密性、水密性、抗风压性"]
[21,"电工套管",6,"外观、尺寸、抗压性能、弯曲性能、等",{"$nulls":5},"1400KN/600KN"]
[22,"压实度",300,"密度、含水率"]
[23,"天然地基承载力",185,"承载力"]
[24,"沥青配合比",1,"配合比"]
[25,"沥青路面检测",12,"厚度、压实度等"]
[26,"挤塑板",1,"燃烧性能"]
[27,"钢筋拉拔",50,"植筋抗拔力"]
[28,"钢筋扫描",120,"保护层厚度、钢筋间距、钢筋根数"]
[29,"种植土",2,"PH值等"]
[30,"室内环境",30,"甲醛、氨、氡、苯、甲苯、二甲苯、TVOC"]
[31,"合计"]